Setting up to use your Epson 7800 or 9800 with CLEAR FOCUS Aqueous Inkjet-compatible Perforated Window Films (JetVue or ImageJetVue)

This profile works with both the 1.5- and 2-mm hole size perforated window films.

Note that this profile is for either an Epson 7800 or a 9800 set up with Matte Black inks only.

Instructions are shown for printing through Photoshop using the Epson Driver. 

Add the profile to the appropriate directory of your PC or Mac.

In Photoshop, after setting up your page size, select Print with Preview.
In the first screen you will see your print space selected, followed by another selection area where you are to select the Eps98k_ClrFocus_1440_WCPRW.icc profile. 

(Note: If the profile doesn't show up, it's been placed in the wrong folder.)

Then Select Print
In the next screen, select from the material list Water Color Paper Radiant White.
Next, using the various menus, select Superfine 1440 High Speed, No color adjustment, and turn off the material cutter.

Finally, select Print.